{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":24,"n_cols":2,"rows_kept":24,"flags":["formulas_cached_only"]}
["PK17 Type "]
[]
["Technical data"]
[]
[null,"● Inductance loss ≤18% DC preload with Isat and ambient temperature 80℃"]
[null,"●  Operating temperature range:-10℃～115℃"]
[null,"●  Normal inductance at 1KHz,1Vac,25℃"]
[null,"●  Inductance tolerance ±30%"]
[null,"●  Customer-specific types on request"]
[]
["Application"]
[]
[null,"● Line fiiter"]
[null,"●  Ballast,switching power supply,etc."]
[null,"●  Low capacity winding design with four chambers"]
[null,"●  Full utilisation of material permeability due to closed core"]
[null,"●  RoHS Compliance"]
[]
["Design PK17"]
[]
[null,"●  Core:PK17"]
[null,"●  Coil former:vertical"]
[]
["Typical configuration & dimensions & Circuit Diagram"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}