{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":2,"rows_kept":22,"flags":["formulas_cached_only"]}
["EF16/7.4 Type "]
[]
["Technical data"]
[]
[null,"●  Typical switching frenquncy 500KHz Max."]
[null,"●  Operating temperature range:-10℃～115℃"]
[null,"●  Normal inductance at 10KHz,1Vac,25℃"]
[null,"●  Inductance tolerance ±5% at gapped core,±30% at ungapped core"]
[null,"●  Customer-specific types on request"]
[]
["Application"]
[]
[null,"● Standby transformers,line filters,inductors,etc."]
[null,"●  Ballast,switching power supply,etc."]
[null,"●  RoHS Compliance"]
[]
["Design EF16/7.4"]
[]
[null,"●  Core:EF16/7.4"]
[null,"●  Coil former:vertical"]
[]
["Typical configuration & dimensions & Circuit Diagram"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}